com.google.zxing.qrcode.decoder

## Enum Mode

- java.lang.Object
- - java.lang.Enum<Mode>
  - - com.google.zxing.qrcode.decoder.Mode

- All Implemented Interfaces:
    Serializable, Comparable<Mode>

      public enum Mode
      extends Enum<Mode>

  See ISO 18004:2006, 6.4.1, Tables 2 and 3. This enum encapsulates the various modes in which data can be encoded to bits in the QR code standard.

  Author:
    Sean Owen

- - ### Enum Constant Summary

    Enum Constants
    Enum Constant and Description
    `ALPHANUMERIC`
    `BYTE`
    `ECI`
    `FNC1_FIRST_POSITION`
    `FNC1_SECOND_POSITION`
    `HANZI` See GBT 18284-2000; "Hanzi" is a transliteration of this mode name.
    `KANJI`
    `NUMERIC`
    `STRUCTURED_APPEND`
    `TERMINATOR`

  - ### Method Summary

    All Methods Static Methods Instance Methods Concrete Methods
    Modifier and Type | Method and Description
    --- | ---
    `static Mode` | `forBits(int bits)`
    `int` | `getBits()`
    `int` | `getCharacterCountBits(Version version)`
    `static Mode` | `valueOf(String name)` Returns the enum constant of this type with the specified name.
    `static Mode[]` | `values()` Returns an array containing the constants of this enum type, in the order they are declared.

    - ### Methods inherited from class java.lang.Enum

      `clone, compareTo, equals, finalize, getDeclaringClass, hashCode, name, ordinal, toString, valueOf`

    - ### Methods inherited from class java.lang.Object

      `getClass, notify, notifyAll, wait, wait, wait`

- - ### Enum Constant Detail

    - #### TERMINATOR

          public static final Mode TERMINATOR

    - #### NUMERIC

          public static final Mode NUMERIC

    - #### ALPHANUMERIC

          public static final Mode ALPHANUMERIC

    - #### STRUCTURED_APPEND

          public static final Mode STRUCTURED_APPEND

    - #### BYTE

          public static final Mode BYTE

    - #### ECI

          public static final Mode ECI

    - #### KANJI

          public static final Mode KANJI

    - #### FNC1_FIRST_POSITION

          public static final Mode FNC1_FIRST_POSITION

    - #### FNC1_SECOND_POSITION

          public static final Mode FNC1_SECOND_POSITION

    - #### HANZI

          public static final Mode HANZI

      See GBT 18284-2000; "Hanzi" is a transliteration of this mode name.

  - ### Method Detail

    - #### values

          public static Mode[] values()

      Returns an array containing the constants of this enum type, in the order they are declared. This method may be used to iterate over the constants as follows:

          for (Mode c : Mode.values())
              System.out.println(c);

      Returns:
        an array containing the constants of this enum type, in the order they are declared

    - #### valueOf

          public static Mode valueOf(String name)

      Returns the enum constant of this type with the specified name. The string must match exactly an identifier used to declare an enum constant in this type. (Extraneous whitespace characters are not permitted.)
      Parameters:
        `name` - the name of the enum constant to be returned.
      Returns:
        the enum constant with the specified name
      Throws:
        `IllegalArgumentException` - if this enum type has no constant with the specified name
        `NullPointerException` - if the argument is null

    - #### forBits

          public static Mode forBits(int bits)

      Parameters:
        `bits` - four bits encoding a QR Code data mode
      Returns:
        Mode encoded by these bits
      Throws:
        `IllegalArgumentException` - if bits do not correspond to a known mode

    - #### getCharacterCountBits

          public int getCharacterCountBits(Version version)

      Parameters:
        `version` - version in question
      Returns:
        number of bits used, in this QR Code symbol `Version`, to encode the count of characters that will follow encoded in this Mode

    - #### getBits

          public int getBits()

Copyright © 2007–2018. All rights reserved.