SNMP-COMMUNITY-MIB DEFINITIONS ::= BEGIN

-- Taken from RFC 2576
--
-- Copyright (C) The Internet Society (1999). All Rights Reserved.
--
-- This document and translations of it may be copied and furnished to
-- others, and derivative works that comment on or otherwise explain it
-- or assist in its implementation may be prepared, copied, published
-- and distributed, in whole or in part, without restriction of any
-- kind, provided that the above copyright notice and this paragraph are
-- included on all such copies and derivative works.  However, this
-- document itself may not be modified in any way, such as by removing
-- the copyright notice or references to the Internet Society or other
-- Internet organizations, except as needed for the purpose of
-- developing Internet standards in which case the procedures for
-- copyrights defined in the Internet Standards process must be
-- followed, or as required to translate it into languages other than
-- English.
--
-- The limited permissions granted above are perpetual and will not be
-- revoked by the Internet Society or its successors or assigns.
--
-- This document and the information contained herein is provided on an
-- "AS IS" basis and THE INTERNET SOCIETY AND THE INTERNET ENGINEERING
-- TASK FORCE DISCLAIMS ALL WARRANTIES, EXPRESS OR IMPLIED, INCLUDING
-- BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE INFORMATION
-- HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED WARRANTIES OF
-- MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.

IMPORTS
    IpAddress,
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Integer32,
    snmpModules
        FROM SNMPv2-SMI
    RowStatus,
    StorageType
        FROM SNMPv2-TC
    SnmpAdminString,
    SnmpEngineID
        FROM SNMP-FRAMEWORK-MIB
    SnmpTagValue,
    snmpTargetAddrEntry
        FROM SNMP-TARGET-MIB
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF;

snmpCommunityMIB MODULE-IDENTITY
    LAST-UPDATED "200003060000Z"          -- 6 Mar 2000, midnight
    ORGANIZATION "SNMPv3 Working Group"
    CONTACT-INFO "WG-email:   snmpv3@lists.tislabs.com
                  Subscribe:  majordomo@lists.tislabs.com
                              In msg body:  subscribe snmpv3

                  Chair:      Russ Mundy
                              TIS Labs at Network Associates
                  Postal:     3060 Washington Rd
                              Glenwood MD 21738
                              USA
                  Email:      mundy@tislabs.com
                  Phone:      +1-301-854-6889



                  Co-editor:  Rob Frye
                              CoSine Communications
                  Postal:     1200 Bridge Parkway
                              Redwood City, CA 94065
                              USA
                  E-mail:     rfrye@cosinecom.com
                  Phone:      +1 703 725 1130

                  Co-editor:  David B. Levi
                              Nortel Networks
                  Postal:     3505 Kesterwood Drive
                              Knoxville, TN 37918
                  E-mail:     dlevi@nortelnetworks.com
                  Phone:      +1 423 686 0432

                  Co-editor:  Shawn A. Routhier
                              Integrated Systems Inc.
                  Postal:     333 North Ave 4th Floor
                              Wakefield, MA 01880
                  E-mail:     sar@epilogue.com
                  Phone:      +1 781 245 0804

                  Co-editor:  Bert Wijnen
                              Lucent Technologies
                  Postal:     Schagen 33
                              3461 GL Linschoten
                              Netherlands
                  Email:      bwijnen@lucent.com
                  Phone:      +31-348-407-775
                 "

        DESCRIPTION
            "This MIB module defines objects to help support coexistence
             between SNMPv1, SNMPv2c, and SNMPv3."
        REVISION "200003060000Z" -- 6 Mar 2000
        DESCRIPTION "This version published as RFC 2576."
        REVISION "199905130000Z" -- 13 May 1999
        DESCRIPTION "The Initial Revision"
    ::= { snmpModules 18 }

-- Administrative assignments ****************************************

snmpCommunityMIBObjects     OBJECT IDENTIFIER ::= { snmpCommunityMIB 1 }
snmpCommunityMIBConformance OBJECT IDENTIFIER ::= { snmpCommunityMIB 2 }

--
-- The snmpCommunityTable contains a database of community strings.
-- This table provides mappings between community strings, and the


-- parameters required for View-based Access Control.
--

snmpCommunityTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF SnmpCommunityEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The table of community strings configured in the SNMP
         engine's Local Configuration Datastore (LCD)."
    ::= { snmpCommunityMIBObjects 1 }

snmpCommunityEntry OBJECT-TYPE
    SYNTAX       SnmpCommunityEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Information about a particular community string."
    INDEX       { IMPLIED snmpCommunityIndex }
    ::= { snmpCommunityTable 1 }

SnmpCommunityEntry ::= SEQUENCE {
    snmpCommunityIndex               SnmpAdminString,
    snmpCommunityName                OCTET STRING,
    snmpCommunitySecurityName        SnmpAdminString,
    snmpCommunityContextEngineID     SnmpEngineID,
    snmpCommunityContextName         SnmpAdminString,
    snmpCommunityTransportTag        SnmpTagValue,
    snmpCommunityStorageType         StorageType,
    snmpCommunityStatus              RowStatus
}

snmpCommunityIndex OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique index value of a row in this table."
    ::= { snmpCommunityEntry 1 }

snmpCommunityName OBJECT-TYPE
    SYNTAX       OCTET STRING
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The community string for which a row in this table
         represents a configuration."
    ::= { snmpCommunityEntry 2 }


snmpCommunitySecurityName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(1..32))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "A human readable string representing the corresponding
         value of snmpCommunityName in a Security Model
         independent format."
    ::= { snmpCommunityEntry 3 }

snmpCommunityContextEngineID OBJECT-TYPE
    SYNTAX       SnmpEngineID
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The contextEngineID indicating the location of the
         context in which management information is accessed
         when using the community string specified by the
         corresponding instance of snmpCommunityName.

         The default value is the snmpEngineID of the entity in
         which this object is instantiated."
    ::= { snmpCommunityEntry 4 }

snmpCommunityContextName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(0..32))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The context in which management information is accessed
         when using the community string specified by the corresponding
         instance of snmpCommunityName."
    DEFVAL      { ''H }   -- the empty string
    ::= { snmpCommunityEntry 5 }

snmpCommunityTransportTag OBJECT-TYPE
    SYNTAX       SnmpTagValue
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "This object specifies a set of transport endpoints
         from which a command responder application will accept
         management requests.  If a management request containing
         this community is received on a transport endpoint other
         than the transport endpoints identified by this object,
         the request is deemed unauthentic.

         The transports identified by this object are specified


         in the snmpTargetAddrTable.  Entries in that table
         whose snmpTargetAddrTagList contains this tag value
         are identified.

         If the value of this object has zero-length, transport
         endpoints are not checked when authenticating messages
         containing this community string."
    DEFVAL      { ''H }   -- the empty string
    ::= { snmpCommunityEntry 6 }

snmpCommunityStorageType OBJECT-TYPE
    SYNTAX       StorageType
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The storage type for this conceptual row in the
         snmpCommunityTable.  Conceptual rows having the value
         'permanent' need not allow write-access to any
         columnar object in the row."
    ::= { snmpCommunityEntry 7 }

snmpCommunityStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
        "The status of this conceptual row in the snmpCommunityTable.

         An entry in this table is not qualified for activation
         until instances of all corresponding columns have been
         initialized, either through default values, or through
         Set operations.  The snmpCommunityName and
         snmpCommunitySecurityName objects must be explicitly set.

         There is no restriction on setting columns in this table
         when the value of snmpCommunityStatus is active(1)."
    ::= { snmpCommunityEntry 8 }

--
-- The snmpTargetAddrExtTable
--

snmpTargetAddrExtTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF SnmpTargetAddrExtEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "The table of mask and mms values associated with the


         snmpTargetAddrTable.

         The snmpTargetAddrExtTable augments the
         snmpTargetAddrTable with a transport address mask value
         and a maximum message size value.  The transport address
         mask allows entries in the snmpTargetAddrTable to define
         a set of addresses instead of just a single address.
         The maximum message size value allows the maximum
         message size of another SNMP entity to be configured for
         use in SNMPv1 (and SNMPv2c) transactions, where the
         message format does not specify a maximum message size."
    ::= { snmpCommunityMIBObjects 2 }

snmpTargetAddrExtEntry OBJECT-TYPE
    SYNTAX       SnmpTargetAddrExtEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
        "Information about a particular mask and mms value."
    AUGMENTS       { snmpTargetAddrEntry }
    ::= { snmpTargetAddrExtTable 1 }

SnmpTargetAddrExtEntry ::= SEQUENCE {
    snmpTargetAddrTMask              OCTET STRING,
    snmpTargetAddrMMS                Integer32
}

snmpTargetAddrTMask OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..255))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The mask value associated with an entry in the
         snmpTargetAddrTable.  The value of this object must
         have the same length as the corresponding instance of
         snmpTargetAddrTAddress, or must have length 0.  An
         attempt to set it to any other value will result in
         an inconsistentValue error.

         The value of this object allows an entry in the
         snmpTargetAddrTable to specify multiple addresses.
         The mask value is used to select which bits of
         a transport address must match bits of the corresponding
         instance of snmpTargetAddrTAddress, in order for the
         transport address to match a particular entry in the
         snmpTargetAddrTable.  Bits which are 1 in the mask
         value indicate bits in the transport address which
         must match bits in the snmpTargetAddrTAddress value.


         Bits which are 0 in the mask indicate bits in the
         transport address which need not match.  If the
         length of the mask is 0, the mask should be treated
         as if all its bits were 1 and its length were equal
         to the length of the corresponding value of
         snmpTargetAddrTable.

         This object may not be modified while the value of the
         corresponding instance of snmpTargetAddrRowStatus is
         active(1).  An attempt to set this object in this case
         will result in an inconsistentValue error."
    DEFVAL { ''H }
    ::= { snmpTargetAddrExtEntry 1 }

snmpTargetAddrMMS OBJECT-TYPE
    SYNTAX      Integer32 (0|484..2147483647)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The maximum message size value associated with an entry
         in the snmpTargetAddrTable."
    DEFVAL { 484 }
    ::= { snmpTargetAddrExtEntry 2 }

--
-- The snmpTrapAddress and snmpTrapCommunity objects are included
-- in notifications that are forwarded by a proxy, which were
-- originally received as SNMPv1 Trap messages.
--

snmpTrapAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The value of the agent-addr field of a Trap PDU which
         is forwarded by a proxy forwarder application using
         an SNMP version other than SNMPv1.  The value of this
         object SHOULD contain the value of the agent-addr field
         from the original Trap PDU as generated by an SNMPv1
         agent."
    ::= { snmpCommunityMIBObjects 3 }

snmpTrapCommunity OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION


        "The value of the community string field of an SNMPv1
         message containing a Trap PDU which is forwarded by a
         a proxy forwarder application using an SNMP version
         other than SNMPv1.  The value of this object SHOULD
         contain the value of the community string field from
         the original SNMPv1 message containing a Trap PDU as
         generated by an SNMPv1 agent."
    ::= { snmpCommunityMIBObjects 4 }

-- Conformance Information *******************************************

snmpCommunityMIBCompliances OBJECT IDENTIFIER
                            ::= { snmpCommunityMIBConformance 1 }
snmpCommunityMIBGroups      OBJECT IDENTIFIER
                            ::= { snmpCommunityMIBConformance 2 }

-- Compliance statements

snmpCommunityMIBCompliance MODULE-COMPLIANCE
    STATUS       current
    DESCRIPTION
        "The compliance statement for SNMP engines which
         implement the SNMP-COMMUNITY-MIB."

    MODULE       -- this module
        MANDATORY-GROUPS { snmpCommunityGroup }

        OBJECT           snmpCommunityName
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunitySecurityName
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityContextEngineID
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityContextName
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityTransportTag
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityStorageType


        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

        OBJECT           snmpCommunityStatus
        MIN-ACCESS       read-only
        DESCRIPTION     "Write access is not required."

    ::= { snmpCommunityMIBCompliances 1 }

snmpProxyTrapForwardCompliance MODULE-COMPLIANCE
    STATUS       current
    DESCRIPTION
        "The compliance statement for SNMP engines which
         contain a proxy forwarding application which is
         capable of forwarding SNMPv1 traps using SNMPv2c
         or SNMPv3."
    MODULE       -- this module
        MANDATORY-GROUPS { snmpProxyTrapForwardGroup }
    ::= { snmpCommunityMIBCompliances 2 }

snmpCommunityGroup OBJECT-GROUP
    OBJECTS {
        snmpCommunityName,
        snmpCommunitySecurityName,
        snmpCommunityContextEngineID,
        snmpCommunityContextName,
        snmpCommunityTransportTag,
        snmpCommunityStorageType,
        snmpCommunityStatus,
        snmpTargetAddrTMask,
        snmpTargetAddrMMS
    }
    STATUS       current
    DESCRIPTION
        "A collection of objects providing for configuration
         of community strings for SNMPv1 (and SNMPv2c) usage."
    ::= { snmpCommunityMIBGroups 1 }

snmpProxyTrapForwardGroup OBJECT-GROUP
    OBJECTS {
        snmpTrapAddress,
        snmpTrapCommunity
    }
    STATUS       current
    DESCRIPTION
        "Objects which are used by proxy forwarding applications
         when translating traps between SNMP versions.  These are
         used to preserve SNMPv1-specific information when


         translating to SNMPv2c or SNMPv3."
    ::= { snmpCommunityMIBGroups 3 }

END
