SNMP-MPD-MIB DEFINITIONS ::= BEGIN

-- Taken from RFC 2572
-- 
-- Copyright (C) The Internet Society (1999). All Rights Reserved.
--
-- This document and translations of it may be copied and furnished to
-- others, and derivative works that comment on or otherwise explain it
-- or assist in its implementation may be prepared, copied, published
-- and distributed, in whole or in part, without restriction of any
-- kind, provided that the above copyright notice and this paragraph are
-- included on all such copies and derivative works.  However, this
-- document itself may not be modified in any way, such as by removing
-- the copyright notice or references to the Internet Society or other
-- Internet organizations, except as needed for the purpose of
-- developing Internet standards in which case the procedures for
-- copyrights defined in the Internet Standards process must be
-- followed, or as required to translate it into languages other than
-- English.
--
-- The limited permissions granted above are perpetual and will not be
-- revoked by the Internet Society or its successors or assigns.
--
-- This document and the information contained herein is provided on an
-- "AS IS" basis and THE INTERNET SOCIETY AND THE INTERNET ENGINEERING
-- TASK FORCE DISCLAIMS ALL WARRANTIES, EXPRESS OR IMPLIED, INCLUDING
-- BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE INFORMATION
-- HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED WARRANTIES OF
-- MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.

IMPORTS
   MODULE-COMPLIANCE, OBJECT-GROUP         FROM SNMPv2-CONF
   MODULE-IDENTITY, OBJECT-TYPE,
   snmpModules, Counter32                  FROM SNMPv2-SMI;

snmpMPDMIB MODULE-IDENTITY
   LAST-UPDATED "9905041636Z"              -- 4 April 1999
   ORGANIZATION "SNMPv3 Working Group"
   CONTACT-INFO "WG-EMail:   snmpv3@lists.tislabs.com
		 Subscribe:  majordomo@lists.tislabs.com
			     In message body:  subscribe snmpv3

		 Chair:      Russ Mundy
			     TIS Labs at Network Associates
		 postal:     3060 Washington Road
			     Glenwood, MD 21738
			     USA
		 EMail:      mundy@tislabs.com
		 phone:      +1 301-854-6889

		 Co-editor:  Jeffrey Case
			     SNMP Research, Inc.
		 postal:     3001 Kimberlin Heights Road
			     Knoxville, TN 37920-9716
			     USA
		 EMail:      case@snmp.com
		 phone:      +1 423-573-1434

		 Co-editor   Dave Harrington
			     Cabletron Systems, Inc.
		 postal:     Post Office Box 5005
			     MailStop: Durham
			     35 Industrial Way
			     Rochester, NH 03867-5005
			     USA
		 EMail:      dbh@ctron.com
		 phone:      +1 603-337-7357

		 Co-editor:  Randy Presuhn
			     BMC Software, Inc.
		 postal:     965 Stewart Drive
			     Sunnyvale, CA 94086
			     USA
		 EMail:      randy_presuhn@bmc.com
		 phone:      +1 408-616-3100

		 Co-editor:  Bert Wijnen
			     IBM T. J. Watson Research
		 postal:     Schagen 33
			     3461 GL Linschoten
			     Netherlands
		 EMail:      wijnen@vnet.ibm.com
		 phone:      +31 348-432-794

		"
   DESCRIPTION  "The MIB for Message Processing and Dispatching"
   REVISION     "9905041636Z"              -- 4 April 1999
   DESCRIPTION  "Updated addresses, published as RFC 2572."
   REVISION     "9709300000Z"              -- 30 September 1997
   DESCRIPTION  "Original version, published as RFC 2272."
   ::= { snmpModules 11 }

-- Administrative assignments ***************************************

snmpMPDAdmin           OBJECT IDENTIFIER ::= { snmpMPDMIB 1 }
snmpMPDMIBObjects      OBJECT IDENTIFIER ::= { snmpMPDMIB 2 }
snmpMPDMIBConformance  OBJECT IDENTIFIER ::= { snmpMPDMIB 3 }

-- Statistics for SNMP Messages *************************************

snmpMPDStats           OBJECT IDENTIFIER ::= { snmpMPDMIBObjects 1 }

snmpUnknownSecurityModels OBJECT-TYPE
   SYNTAX       Counter32
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION "The total number of packets received by the SNMP
		engine which were dropped because they referenced a
		securityModel that was not known to or supported by
		the SNMP engine.
	       "
   ::= { snmpMPDStats 1 }

snmpInvalidMsgs OBJECT-TYPE
   SYNTAX       Counter32
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION "The total number of packets received by the SNMP
		engine which were dropped because there were invalid
		or inconsistent components in the SNMP message.
	       "
   ::= { snmpMPDStats 2 }

snmpUnknownPDUHandlers OBJECT-TYPE
   SYNTAX       Counter32
   MAX-ACCESS   read-only
   STATUS       current
   DESCRIPTION "The total number of packets received by the SNMP
		engine which were dropped because the PDU contained
		in the packet could not be passed to an application
		responsible for handling the pduType, e.g. no SNMP
		application had registered for the proper
		combination of the contextEngineID and the pduType.
	       "
   ::= { snmpMPDStats 3 }

-- Conformance information ******************************************

snmpMPDMIBCompliances OBJECT IDENTIFIER ::= {snmpMPDMIBConformance 1}
snmpMPDMIBGroups      OBJECT IDENTIFIER ::= {snmpMPDMIBConformance 2}

-- Compliance statements

snmpMPDCompliance MODULE-COMPLIANCE
   STATUS       current
   DESCRIPTION "The compliance statement for SNMP entities which
		implement the SNMP-MPD-MIB.
	       "

   MODULE    -- this module
       MANDATORY-GROUPS { snmpMPDGroup }

   ::= { snmpMPDMIBCompliances 1 }

snmpMPDGroup OBJECT-GROUP
   OBJECTS {
	     snmpUnknownSecurityModels,
	     snmpInvalidMsgs,
	     snmpUnknownPDUHandlers
	   }
   STATUS       current
   DESCRIPTION "A collection of objects providing for remote
		monitoring of the SNMP Message Processing and
		Dispatching process.
	       "
   ::= { snmpMPDMIBGroups 1 }

END
